This file is for defaults for SEISAN and called SEISAN.DEF. The name must
be in upper case on Sun. The following shows the parameters which can be set.
The file can contain any lines in any order, only the lines with 
recognized keywords and a non blank field under Par 1 will be read. The
comments have no importance.

*********NEVER USE TABS IN THIS FILE, IT WILL NOT WORK*****************

KEYWORD............Comments.............Par 1.....Par 2
WAVEFORM_BASE      Waveform base name   NSS
WAVEFORM_BASE      Waveform base name   RUND
WAVEFORM_BASE      Waveform base name   JMI
WAVEFORM_BASE      Waveform base name   TEST
#
#   seisan cont dat abase
#
CONT_BASE          REA continuous base  RUND
CONT_BASE          REA continuous base  JMI
CONT_BASE          REA continuous base  NSS
CONT_BEFORE        start min before     20.
CONT_AFTER         start min after      1.
#
# position in file name where year yyyy and month mm starts
#
CONT_YEAR_MONTH_POSTION_FILE           
#
# archive
#
ARC_CHAN                                SFJD LHZIU10
ARC_CHAN                                KBS  LHZGE10
ARC_CHAN                                DAG  LHZGE
ARC_CHAN                                TULEGLHZDK
ARC_CHAN                                BSD  LHZDK
ARC_CHAN                                BORG LHZII10        20020101  20150202
ARC_ARCHIVE                             ./archive                         
ARC_DURATION                            10000.0
ARC_START_TIME                          100.0
ARC_TYPE                                1.0                        
ARC_BY_DEFAULT                          0.0      

# 
# virtual networks                      NAME      SCNL
# several networks can be defined
#
ARC_VIRTUAL_NETWORK                     _DK       BSD  LHZDK  
ARC_VIRTUAL_NETWORK                     _NO       KBS  LHZGE10
# ... 

#      
# PREM velocity and density model, Q model not known, Q is average along path,
# not Q in layer. Q might be distance dependent. Kappas are low values.
#
SPEC KAPPA p and kappa s                0.01        0.02
SPEC Q BELOW 1 HZ, P,S                  1.0         1.0
#
#                                      depth  vp   vs  Q0p  Qal  Q0s  Qal dens
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      3.0  5.8  3.2  500. 0.7  400. 0.7  2.6 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      15.0 6.8  3.9  500. 0.7  400. 0.7  2.9 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      24.0 8.1  4.5  500. 0.7  400. 0.7  3.4 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      80.0 8.1  4.5  500. 0.7  400. 0.7  3.4
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      171. 8.0  4.4  500. 0.7  400. 0.7  3.4 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      220. 8.6  4.6  500. 0.7  400. 0.7  3.4 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      271. 8.7  4.7  500. 0.7  400. 0.7  3.5 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      371. 8.9  4.8  500. 0.7  400. 0.7  3.5
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      400. 9.1  4.9  500. 0.7  400. 0.7  3.7 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      471. 9.5  5.1  500. 0.7  400. 0.7  3.8 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      571. 10.0 5.4  500. 0.7  400. 0.7  3.9 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      600. 10.2 5.5  500. 0.7  400. 0.7  4.0  
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      670. 10.3 5.6  500. 0.7  400. 0.7  4.0 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      771. 11.1 6.2  500. 0.7  400. 0.7  4.4 
SPEC MODEL h,vp,vs,qp,qap,qs,qas,d      871. 11.2 6.3  500. 0.7  400. 0.7  4.5 

CURSOR             0: default, 1: cross 1.
FOCMEC MAXSOL      max solutions        125.

WAVEFORM_DIRS      Waveform drectory    /net/seismo/seismo/WOR/seisnet
MERGE_WAVEFORM     Code for merging wa  NSN
MAP_LAT_BORDER     dist from center       3.0
MAP_LON_BORDER          "                 6.0
EPIMAP_STATIONS    plot stations
EPIMAP_MAP_FILE    name of map          EUROPE 
EEV_COMMENT        comment for EEV      Depth has benn fixed to 10 km
EEV_COMMENT        comment for EEV      Depth has been fixed to 20 km
EPIMAP_PROJECTION  number                  3.
SPECTRAL GEO_DEPTHS                     10.0       14.0
HERKIJ_DISTANCE                         100.0
REG_KEEP_AUTO      keep phases when reg    1.
COPY_WAV_DIR       copy when register   

TEXT_PRINT               Unix example   nenscript -Psps
OUTPUT_DIR                              ./
INIT_IMGMAP_FILE         PC example     c:/seismo/DAT/IMGWORLD.gif
MAP_SERVER                              0
IMGMAP_PATH              PC example     c:/seismo/DAT/IMGMAP
INIT_MAP_LOWER_LATITUDE                 -90.0
INIT_MAP_UPPER_LATITUDE                 90.0
INIT_MAP_LEFT_LONGITUDE                 -180.0
INIT_MAP_RIGHT_LONGITUDE                180.0
INTERNET_BROWSER         Unix example   /prog/netscape
ACROBAT_READER           PC example     C:\Program Files\Adobe\Acrobat 5.0\Reader\AcroRd32
HELP_DIR                 PC   example   c:/seismo/INF
WEBMAPSERVER2                           http://pcseis6.ifjf.uib.no:7001/getImageMap?ACTION=2&
WEBMAPSERVER3                           http://demo.cubewerx.com/demo/cubeserv/cubeserv.cgi?

# order to select magnitudes as given here from top (high priortiy) to bottom (low priority)
MAGNITUDE_ORDER                         WGCM
MAGNITUDE_ORDER                         LBER
MAGNITUDE_ORDER                         WBER

# parameters for gmap used within eev
GMAP_DIR                                c:/seismo/WOR
GMAP_TYPE                               MAP          [MAP, SATELLITE, HYBRID, TERRAIN]

# parameters for gmap
GMAP_ICON_QUAKE                         http://maps.google.com/mapfiles/kml/pal2/icon26.png
GMAP_ICON_EXPLOSION                     http://maps.google.com/mapfiles/kml/shapes/star.png
GMAP_ICON_PROB_EXPL                     http://maps.google.com/mapfiles/kml/shapes/open-diamond.png
GMAP_ICON_OTHER_EVENTS                  http://maps.google.com/mapfiles/kml/shapes/square.png
GMAP_ICON_MSIZE                         0.5
GMAP_ICON_XSIZE                         0.2
GMAP_ICON_YSIZE                         0.5
#GMAP_APPEND_KML                         <!-- lines to be appended to the gmap.kml file : -->
GMAP_APPEND_KML                         <ScreenOverlay id="LOGO">
GMAP_APPEND_KML                         <name>Info and links</name>
GMAP_APPEND_KML                         <description> <![CDATA[
GMAP_APPEND_KML                         Data is in Nordic format. The format is <br>
GMAP_APPEND_KML                         described in the Seisan manual at UIB.<br>
GMAP_APPEND_KML                         UIB:  http://www.geo.uib.no/seismo/<br> ]]>
GMAP_APPEND_KML                         </description>
GMAP_APPEND_KML                         <Icon>
GMAP_APPEND_KML                          <href>http://seis.geus.net/geus.png</href>
GMAP_APPEND_KML                         </Icon>
GMAP_APPEND_KML                         <overlayXY x="0" y="1" xunits="fraction" yunits="fraction"/>
GMAP_APPEND_KML                         <screenXY x="-0.01" y="0.99" xunits="fraction" yunits="fraction"/>
GMAP_APPEND_KML                         <rotationXY x="0" y="0" xunits="fraction" yunits="fraction"/>
GMAP_APPEND_KML                         <size x="0.1" y="0.1" xunits="fraction" yunits="fraction"/>
GMAP_APPEND_KML                         </ScreenOverlay>
#GMAP_APPEND_KML                         <!-- end of appended lines -->

# parameters for automatic gmap
GMAP_AUTO      0: no, 1:yes             1.0
GMAP_AUTO_ICON_EVENT                    http://maps.google.com/mapfiles/kml/pal2/icon26.png
GMAP_AUTO_ICON_COLOR                    ff0000ff
GMAP_AUTO_ICON_MSIZE                    0.5
GMAP_AUTO_ICON_XSIZE                    0.2
GMAP_AUTO_ICON_YSIZE                    0.5
GMAP_AUTO_LOOKAT_ALTITUDE               2000000.0
GMAP_AUTO_SHOW_STAT  0: no, 1:yes       1.
GMAP_AUTO_ERROR_ELLIPSE  0: no, 1:yes   1.
GMAP_AUTO_STAT_SIZE                     1.1
GMAP_AUTO_STAT_URL                      http://maps.google.com/mapfiles/kml/shapes/triangle.png
GMAP_AUTO_STAT_RESIDAL_GOOD             0.5
GMAP_AUTO_STAT_RESIDUAL_BAD             1.5
GMAP_AUTO_STAT_COLOR_GOOD               ff00ff00
GMAP_AUTO_STAT_COLOR_OK                 ff00ffff
GMAP_AUTO_STAT_COLOR_BAD                ff0000ff
GMAP_AUTO_SHOW_OLD_LOCATION 0:no,1:yes  1.
GMAP_AUTO_OLD_LOCATION_COLOR            ffff0000
GMAP_AUTO_SHOW_PATH   0: no, 1:yes      1.
GMAP_AUTO_PATH_COLOR                    ff929292
GMAP_AUTO_PATH_WIDTH                    2.5
GMAP_AUTO_FILE_ACTION  0: no, 1:yes     0.
GMAP_AUTO_ACTION                        cp gmap.cur.kml /inetpub/www/html/seismo/nnsn
# e.g. GMAP_AUTO_ACTION    ncftpput -u seismo -p passwd ftp.server /home/seismo/www gmap.cur.kml

# Parameters for showing type P files in EEV
PLOT_PDF_COMMAND       for linux        evince  
#PLOT_PDF_COMMAND       for windows      start acrord32.exe
PLOT_PICTURE_COMMAND   for linux        display
#PLOT_PICTURE_COMMAND   for windows      \Programfiler\irfanview\i_view32 



