This file is for defaults for MULPLT and called MULPLT.DEF. The name must
be in upper case on Sun. The following shows the parameters which can be set.
The file can contain any lines in any order, only the lines with 
recognized keywords and a non blank field under Par 1 will be read. The
comments have no importance.

*********NEVER USE TABS IN THIS FILE, IT WILL NOT WORK*****************

KEYWORD............Comments.............Par 1.....Par 2
X_SCREEN_SIZE      Size in % of screen   90.0
PHASE NAME KEY     Phase key and phase                    
PHASE NAME KEY                          
PHASE WEIGHT KEY   Weight key and weight                     
PHASE MOUSE KEY    Mouse key character
NCHAN PER SCREEN   # chan pr screen
SPECTRAL Q0        Q0                    440.0 
SPECTRAL QALPHA    Q = Q0**Qalpha        0.70 
SPECTRAL KAPPA                            
SPECTRAL P-VELOCITY P velocity            6.2 
SPECTRAL S-VELOCITY P velocity            3.6
SPECTRAL DENSITY   Density
SPECTRAL MODEL      0 no 1 yes            1.0
3COMP VELOCITY     velocity for 3 comp
RESOLUTIONX        # points pl. screen  1500.0
RESOLUTIONHC       # points pl. hc      3000.0
NSORT_DISTANCE     0: no sort, min ph.     
SPECTRAL F-BAND    Band to show          0.01     20.0
SPECTROGRAM COMMAND                     /nnsn/prog/obspy/obspy/signal/spectro.py
AUTO_LOCATE        0,1,2       0,1,2     0.0      2.0
AUTO_PROCESS       0,1,2       name      0.0      ls 
SPECTRAL OUTPUT    Makes a file                      1.0
ML LOW CUT AND POLES                     
ML HIGH CUT AND POLES                   
BANDPASS FILTER                                       
AUTOCODA FILTER                          0.1      10.0
AUTOCODA STA                             3.0
AUTOCODA RATIO                           1.2
CODA AUTO                                0.0 
MULPLT WAV OUT FORMAT  Output format     SEISAN
PHASE NAME KEY
PHASE MOUSE KEY
### Set Filter type 0 for bndpas 1 for recfil routine
FILTER TYPE                             0.0
### Setup user-defined filters
FILTER 1                                0.01      0.1
FILTER 2                                0.1       1.0
FILTER 3                                1.0       5.0
FILTER 4                                5.0       10.0
FILTER 5                                10.0      15.0
FILTER 6                                15.0      25.0
FILTER 7                                2.0       4.0
### Magnitude filters
MULPLT AREA                             0.0
MULPLT LAT LON                          60.0      5.0
MULPLT RADIUS                           2.0
MULPLT STAT                             BER
###
#DEFAULT CHANNEL                         TRO       S  Z
